

1.Please see the picture(①), which is the PlatformIO plugin, and then click ② Open Project to open the project.




Find the BIGTREETECH TFT35 firmware source directory , then click Open




After opening the project, go to the platformio.ini file and change the default environment .

the “env\_default” can be “BIGTREE\_TFT35\_V1\_2”, “BIGTREE\_TFT35\_V1\_1”, and “BIGTREE\_TFT35\_V1\_0”

it depends on your hardware.



After the modification is complete, press Ctrl+Alt+B, and platformio will automatically download the compiled component and compile it.



After the compilation is successful, a BIQU\_TFT35\_V1.x.x.bin file will be generated in the .pioenvs\BIGTREE\_TFT35\_V1\_x directory. We need copy this file to the SD card, and insert this SD Card to TFT35 Touch Screen, then reset the Touch Screen, the firmware will be updated automatically.